MUGBERIA GANGADHAR MAHAVIDYALAYA

P.O. Bhupatinagar, Dist. Purba Medinipur

 Memo No.:MGM/Material Supply/Labour Con./ **234**/2017-18, Dt: 02/02/18.

**NOTICE INVITING QUATATION**

 Sealed quotation are invited from renowned and bonafied suppliers for supplying the following Materials/and Labour Contractor for the following Materials / Works of Mugberia Gangadhar College Building at Bhupatinagar Dist. PurbaMedinipur.

 MATERIALS :-

1. Floor Tiles
2. Aluminum sliding shutters
3. False Ceiling
4. Paints
5. Ceiling Fans

LABOUR CONTRACT:-

1. Painting Works
2. Fitting and Fixing of Floor Tiles

Quotations are to be quoted for each of these items separately.

For details visit college website: [www.mugberiagangadharmahavidyalaya.org](http://www.mugberiagangadharmahavidyalaya.org).

Last date of submission: **12/02/2018**

 Sd/-

PRINCIPAL

 Mugberia Gangadhar Mahavidyalaya

 **9002275816**

**Materials and Works details of the above mentioned Quotations**

**A MATERIALS:-**

1. Supplying, fitting and fixing 1st quality ceramic tiles(Kazaria-6002)

 in walls and floors & 4 Nos. of key stones (10 mm) fixed

 With araldite at the back of each tile and finishing the

Joints with white cement mixed with coloring oxide (if

required) to match the colour of tiles including

roughening of concrete surfaces, if necessary or by

synthetic adhesive & grout materials etc. **: @ /per Sq.mt.**

2. Supplying, fitting & fixing of 2-Track/3-Track Aluminum

 Sliding Window of all Aluminum sections viz. window frame

 (top, bottom & side frame), shutter (top, bottom, side & interlock

 member) made of aluminum alloy extrusions conforming

to IS 733-1983 & IS 1285-1975, annodised conforming to IS

1868-1983, fitted with all other accessories viz. PVC roller,

EPDM gasket, maruti lock, screws etc. including labour charges

For fitting & fixing of aluminum 2-track/3-track sliding window

With fixing of glass (excluding cost of glass) all complete as per

Architectural drawings and direction of Engineer-in-charge.

10-12 Micron thickness Anodizing film Natural white.

***For 2-Track window:*** Members for Bottom frame @ 0.875 Kg

Per Mtr. And for Top and Side frame @ 0.778 Kg per Mtr.

And for shutter Bottom and Top member @ 0.472 Kg per Mtr.

Style side member @ 0.493 Kg per Mtr. And Interlock member

@ 0.612 Kg per Mtr.

***For 3-Track window***: Members for Bottom frame @ 1.233 Kg per

Mtr. And for Top and Side frame @ 1.067 Kg per Mtr. And for shutter

Bottom and Top member @ 0.472 Kg per Mtr., Style side member

@0.493 Kg per Mtr. And Interlock member @ 0.612 Kg per Mtr**.: @ / Kg.**

3. Supplying bubble free float glass of approved make and brand

 Conforming to IS: 2835-1987. : **@ / Sq.mt.**

4. Supplying M.S. or W.I. ornamental grill of Approved

 design joints continuously welded with M.S., W.I. flats,

 bars, shoes & pipes for stair railing fitted and fixed with

 necessary screws and lugs. : @ /Kg

5. PAINTS:-(Asian Paints Co.)

 i) Exterior grade acrylic primer **: @ /Ltr.**

 ii) Oil bound Primer **: @ /Ltr.**

iii) Metal Primer **: @ /Ltr.**

 iv) Acrylic Distemper : **@ /Ltr.**

 v) Exterior Emulsion paint **: @ /Ltr.**

 vi) Synthetic paint **: @ /Ltr.**

Contd.. P/2

Page: 2

6. 48" Ceiling Fans (Crompton Greaves Co) – Brown Colour **: @ /each**

7. A) Supplying fitting & fixing concealed False ceiling Framework

 With G.I. Section (perimeter channels having one flange of 20

 mm. and another flange lof 30 mm. with thickness of 0.55 mm.

 and web of length 27 mm., along the perimeter of the ceiling,

 screws fixed to the wall with help of nylon sleeves or PVC dash

 fasteners @ 610 mm. c/c. then suspend G.I. intermediate “C”

 section with web 90 mm. and flanges of 15 mm. each from

 soffit @ 1200 mm. c/c with ceiling angle of size 25 mm.

 X 10 mm. X 0.55 mm. thickness having web of 51.5 mm. and

 Two flanges of 26 mm each with lips of 10.55 mm., are then fixed

 On to the intermediate channel with the help of connecting clips

 In the direction perpendicular to the intermediate channel

 @ 610 mm. c/c) with fully threaded fiber cement screws

 @ 300 mm. c/c. al complete as per the drawing and direction

 of Engineer-in-charge.

 Section specification:- Perimeter Channel :- 30 mm X 20 mm.

 Thickness 0.55 mm (min), Intermediate Channel :- 15 mm X 90 mm,

 Thickness 0.90 mm (mini), Ceiling Section :- 51.5 mm X 26 mm X

 10.55 mm. thickness 0.55 mm (min),

 Ceiling Angle :- 25 mm X 10 mm. thickness 0.55 mm (min). **: @ /Sq.mt.**

 B) Supplying fitting & fixing Eco-friendly, Moisture Resistant

 And Incombustible Gypsum plaster board tiles (Density >

 700 Kg per Cu.m) conforming to IS 2095-Part-I, 2011 of size

 595 mm x 595 mm. of approved design and brand placed in

 the Grid module to form a false ceiling all complete as per

 drawing & direction of Engineer-in-charge

 ii) 12.5 mm thick Square edged Gypsum Plaster Board / tiles **: @ /Sq.mt.**

**B. LABOUR CONTRACT :-**

1. Acrylic Distemper to interior wall, ceiling with a coat of

 Solvent based interior grade acrylic primer (as per

 manufacturer’s specification) including cleaning and

 smoothening of surface.

 **Two Coats : @ /Sq.mt.**

2. Applying Exterior grade Acrylic primer of approved

 Quality and brand on plastered or concrete surface old or

 new surface to receive acrylic exterior emulsion paint

 including scrapping and preparing the surface thoroughly,

 complete as per manufacturer’s specification and

 direction of the Engineer-in-charge at all elevation.

 ----- ----- one coats. **At First Floor : @ /Sq.mt.**

 Contd. ….P/3

**Page: 3**

3. Protective and decorative Acrylic Finish Exterior

 emulsion Paint of approved quality, as per

 manufacturer’s specification and as per direction of

 Engineer-in-charge to be applied over a acrylic primer as

 required. The rates includes the cost of materials, labour,

 scaffolding and all others incidental charges but

 excluding the cost of primer.

 Two or more coats to give an even shade.

 Premium 100% Acrylic Emulsion. **At First Floor : @ /Sq.mt.**

4. (a) Priming one coat on timber or plastered surface with

 synthetic, oil bound primer of approved quality including

 smoothening surfaces by sand papering etc. **: @ /Sq.mt.**

 (b) Priming one coat on steel or other metal surface with

 synthetic oil bound primer of approved quality including

 smoothening surfaces by sand papering etc. **: @ /Sq.mt.**

5. Painting with best quality synthetic enamel paint of

 approved make and brand including smoothening

 surface by sand papering etc. including using of

 approved putty etc. on the surface, if necessary.

1. On timber or plastered surface:

Two coats (with any shade except white) **: @ /Sq.mt.**

 (b) On steel or other metal surface :

 With super gloss (hi-gloss) –

 (iv) Two coats (with any shade except white) **: @ /Sq.mt.**

6. LABOUR Charges for Fitting & Fixing of

Vitrified Tiles **: @ /Sq.mt.**

Sd/-

PRINCIPAL

 Mugberia Gangadhar Mahavidyalaya

 **9002275816**